|  |  |  |
| --- | --- | --- |
| **Type** | **Part Description** | **Quantity** |
| Breadboard | Solderless, 830 Tie Points, 4 Power Rails | 1 ea |
| IC, DIP-8 | LM/UA741, Single Op Amp | 2 ea |
| IC, DIP-8 | TLE2061, BiFET, High-Output, Single Op Amp IC | 2 ea |
| IC, DIP-8 | TL026, Differential Op Amp IC | 2 ea |
| IC, DIP-14 | TL071, JFET Dual Op Amp IC | 2 ea |
| Transistor | 2N3904, NPN, GP Switch/Amplifier, TO-92 | 4 ea |
| Transistor | 2N3906, PNP, GP Switch/Amplifier, TO-92 | 4 ea |
| Diode | 1N4001, 100V, 1 Amp, Silicon, Power | 5 ea |
| Diode | 1N4004, 400V, 1 Amp, Silicon, Power | 5 ea |
| Diode | 1N4148, Silicon, Signal | 5 ea |
| Zener Diode | 1N751, 5.1V, 500mWatt, Axial, DO-35 | 5 ea |
| Zener Diode | MA7150B, 15V, 800mWatt, Axial | 5 ea |
| Zener Diode | BZX55C18, 18V, 500mWatt, Axial | 5 ea |
| Resistor | 5.1 Ohms, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 13 Ohms, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 22 Ohms, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 68 Ohms, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 100 Ohms, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 240 Ohms, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 330 Ohms, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 470 Ohms, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 560 Ohms, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 750 Ohms, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 1.0K, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 1.8K, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 2.4K, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 5.6K, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 8.2K, 1/2 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 11K, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 15K, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 24K, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 43K, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 51K, 1/2 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 100K, 1/2 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 150K, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 270K, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 430K, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Resistor | 1.5M, 1/4 Watt, 5%, Carbon Film | 5 ea |
| Capacitor | 7.5pF, 50v, NPO, Ceramic Disc | 2 ea |
| Capacitor | 15pF, 50v, NPO, Ceramic Disc | 2 ea |
| Capacitor | 33pF, 50v, NPO, Ceramic Disc | 2 ea |
| Capacitor | 220pF, 50v, NPO, Ceramic Disc | 2 ea |
| Capacitor | 470pF, 50v, NPO, Ceramic Disc | 2 ea |
| Capacitor | 820pF, 50v, NPO, Ceramic Disc | 2 ea |
| Capacitor | 1200pF, 250v, Metal Polyester | 2 ea |
| Capacitor | 2200pF, 50v, X5F, Ceramic Disc | 2 ea |
| Capacitor | .022uF, 50v, X7R, Ceramic Disc | 2 ea |
| Capacitor | .033uF, 250v, Metal Polyester | 2 ea |
| Capacitor | .056uF, 50v, X7R, Ceramic Disc | 2 ea |
| Capacitor | .15uF, 50v, X7R, Ceramic Disc | 2 ea |
| Capacitor | .47uF, 63v, 85° C, Aluminum, Radial | 2 ea |
| Capacitor | 4.7uF, 25v, 85° C, Aluminum, Radial | 2 ea |
| Capacitor | 6.8uF, 35v, 85° C, Aluminum, Radial | 2 ea |
| Capacitor | 10uF, 16v, 85° C, Aluminum, Radial | 2 ea |
| Capacitor | 33uF, 10v, 85° C, Aluminum, Radial | 2 ea |
| Capacitor | 68uF, 16v, 85° C, Aluminum, Radial | 2 ea |
| Capacitor | 100uF, 16v, 85° C, Aluminum, Radial | 2 ea |
| Capacitor | 120uF, 25v, 85° C, Aluminum, Radial | 2 ea |
| Capacitor | 330uF, 25v, 85° C, Aluminum, Radial | 2 ea |
| Capacitor | 1200uF, 10v, 85° C, Aluminum, Radial | 2 ea |
| Capacitor | 2200uF, 16v, 85° C, Aluminum, Radial | 2 ea |
| Capacitor | 3900uF, 6.3v, 85° C, Aluminum, Radial | 2 ea |
| Capacitor | 3.3uF, 25V, Tantalum, Radial | 2 ea |
| Capacitor | 15uF, 16V,Tantalum, Radial | 2 ea |
| Capacitor | 33uF, 6V, Tantalum, Radial | 2 ea |
| Crystal | 4.9152 MHz, HC-49U | 1 ea |
| Crystal | 7.3728 MHz, HC-49U | 1 ea |
| Crystal | 13.500 MHz, HC-49U | 1 ea |
| Clock Oscillator | 50.000 MHz, DIP-4 | 1 ea |
| Inductor | 12uH, Radial | 2 ea |
| Inductor | 100uH, Axial | 2 ea |
| Inductor | 220uH, Axial | 2 ea |
| Inductor | 1.0mH, Axial | 2 ea |
| LED | Bi-Color, Red & Green, Diffused | 2 ea |
| LED | Red, Bright, Round, 5mm | 3 ea |
| LED | Green, Bright, Round, 5mm | 3 ea |
| LED | Yellow, Bright, Round, 5mm | 3 ea |
| LED | Blue, Bright, Round, 5mm | 3 ea |
| LED | White, Bright, Round, 5mm | 3 ea |
| Potentiometer | 470 Ohms, Single-Turn, PCB Mount | 1 ea |
| Potentiometer | 1.0K, Single-Turn, PCB Mount | 1 ea |
| Potentiometer | 22K, Single-Turn, PCB Mount | 1 ea |
| Potentiometer | 100K, Single-Turn, PCB Mount | 1 ea |
| Potentiometer | 220K, Single-Turn, PCB Mount | 1 ea |
| Potentiometer | 320K, Single-Turn, PCB Mount | 1 ea |
| Potentiometer | 1.0M, Single-Turn, PCB Mount | 1 ea |
| Battery Clip | 9V, Snap-type, 2 wires | 1 ea |
| Speaker | 8 Ohms, .1 Watt, Round, Miniature | 1 ea |
| Switch | Pushbutton, SPST Momentary, PCB Mount | 2 ea |
| Switch | Slide, SPDT Momentary, PCB Mount | 2 ea |
| Microphone | Electret, Panasonic | 1 ea |
| Header | Male, 8-pin .100" Centers, Square Post, Breakable | 1 ea |
| Jumper | Shorting Plug for Header, .100" Spacing | 2 ea |